{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["样例","Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"样例","index":0,"n_rows":6,"n_cols":12,"rows_kept":6,"merged":[[0,0,0,11],[5,3,13,11]],"flags":["formulas_cached_only"]}
["单位盖章（）                                                项目名称：  XXXX实验室XXXX省部共建项目设备标书"]
["分包号","单位","设备序号","设备名称","数量","单位","单价(元)","总价(万元)","拟选厂家/型号","详细技术指标及配(附)件","询价依据","备注"]
[1,"化学",1,"中央台",4,"套",10080,4.032,"兰州XXXX公司\n\n西安XXXX公司\n\n青海XXXX公司","1、 主框架","1309911XXXX\n\nXXXX（XX经理）","XXX"]
[1,"化学",2,"台式电脑",2,"台",0.55,55,"兰州XXXX公司\n\n西安XXXX公司\n\n青海XXXX公司","Pentium D 915","网上查询"]
[]
[{"$nulls":3},"1.每项设备只占一行；\n2.不得合并表格\n3.除所列栏目外，其他事项均填入备注栏\n4.凡实验台项目均要求有图样\n5.拟选厂家/型号应是设备生产厂家及型号\n6.书面标书要求单位负责人签名确认，单位盖章。并同时报电子版\n7.可参照样例，如有疑问，请与实验室管理处杨老师联系（Tel:5310951）\n"]

{"sheet":"Sheet1","index":1,"n_rows":18,"n_cols":5,"rows_kept":18,"merged":[[0,0,0,4],[4,0,7,0],[8,0,9,0],[10,0,11,0],[12,0,16,0],[17,0,17,4]],"flags":["formulas_cached_only"]}
["天河工程校内基地建设标书"]
["设备序号","设备名称","数量","单位","详细技术指标及配(附)件"]
["1-前期工程","打拆地面",408,"m2","原有地面打毛处理，提高与上层水泥的粘合能力。"]
["2-水电部分","电路改造",204,"m2","1、走墙内套PVC管、过梁柱用黄腊管、线在途中不能有接头。                                                                                      2、接头套黄腊管及电胶布保护、线路走向横平竖直，不能走弯线。                                                             3    众邦电线2.5mm2单芯铜线。注意：此项结算数可能与报价相差较大,（不含主电缆线）。"]
["3-泥土部分","水泥地面找平",204,"m2","1、大通牌32.5＃水泥及人工                                                                                                                     2、厚度超过3公分另计算地面找平。                                                                                                "]
[null,"地面瓷砖铺贴",204,"m2","1、按要求留缝、垂直、面平、对缝。                                                                                                                           2、大通牌32.5＃水泥及人工，（不含地砖）。                                                                                                          3、厚度超过3公分另计算地面找平。                                                                                                "]
[null,"砌24分砖墙",60,"m2","1、须经物业同意，客户负责办理有关手续。                                                                                                     2、使用轻质砖，强度大通牌325#水泥砂浆砌筑                                        "]
[null,"墙面批灰",120,"m2","双面水泥砂浆批荡。 "]
["4-木工部分","隔墙",136,"m2","轻钢龙骨木工板+泰山牌石膏板隔墙"]
[null,"立柜",4,"m2","满足放置功放，交换机等设备，美观。"]
["5-油漆、灰土部分","腻子粉打底",556,"m2","1、原墙面清理;腻子粉、批刮底灰一遍、面灰二遍，打磨平整。（如需要108胶水另计4元／m2)"]
[null,"漆饰面",556,"m2","1. 底漆二遍，面漆一遍。                                                                                                                                                                                                                                             "]
["6-主材","瓷砖",204,"m2","800*800玻化砖"]
[null,"电地暖",204,"m2","电地暖"]
[null,"保温",287,"m2","BS-A防火A级保温材料"]
[null,"开关插座",1,"项","开关插座"]
[null,"双开门",2,"樘","木门 , 宽×高＝1500×2100mm"]
["报名前，需要现场勘验，联系人：柏老师，15500541626"]